Reader SuccessFully Connected

MotoC1G2BlockPermalockOpSpecResult failed: The Tag does not support error-specific codes

MotoC1G2BlockPermalockOpSpecResult failed: The Tag does not support error-specific codes

ADD\_ACCESSSPEC: Error in parameter Type: 453 for field: 2

Set Mask Data :8000

Permalock on MemBank :MEMORY\_BANK\_USER readback Mask :8000

C1G2WriteOpSpecResult failed: Tag Memory Locked

Perma Lock Success

Set Mask Data :4000

Permalock on MemBank :MEMORY\_BANK\_USER readback Mask :C000

C1G2WriteOpSpecResult failed: Tag Memory Locked

Perma Lock Success

Set Mask Data :2000

Permalock on MemBank :MEMORY\_BANK\_USER readback Mask :E000

C1G2WriteOpSpecResult failed: Tag Memory Locked

Perma Lock Success

Set Mask Data :1000

Permalock on MemBank :MEMORY\_BANK\_USER readback Mask :F000

C1G2WriteOpSpecResult failed: Tag Memory Locked

Perma Lock Success

Set Mask Data :0800

Permalock on MemBank :MEMORY\_BANK\_USER readback Mask :F800

C1G2WriteOpSpecResult failed: Tag Memory Locked

Perma Lock Success

Set Mask Data :0400

Permalock on MemBank :MEMORY\_BANK\_USER readback Mask :FC00

C1G2WriteOpSpecResult failed: Tag Memory Locked

Perma Lock Success

Set Mask Data :0200

Permalock on MemBank :MEMORY\_BANK\_USER readback Mask :FE00

C1G2WriteOpSpecResult failed: Tag Memory Locked

Perma Lock Success

Set Mask Data :0100

Permalock on MemBank :MEMORY\_BANK\_USER readback Mask :FF00

C1G2WriteOpSpecResult failed: Tag Memory Locked

Perma Lock Success

Reader SuccessFully DisConnectedBUILD SUCCESSFUL (total time: 4 minutes 30 seconds)